More External Components/Domains
Prev | Chapter 60. Basic Configuration Options (External Component) | Next

## More External Components/Domains

Suppose you want to connect more than one external component. Let’s say you want to connect PubSub and MSN components to the Tigase server as well.

In such a case you don’t have to open another port on the server. All the components can connect to the same port. Of course each of the components connect for a different domain and probably should use a different password.

Let’s say then that we want the Tigase server accept two more domains with corresponding passwords: (pubsub.devel.tigase.org:pubsub_pass) and (msn.devel.tigase.org:msn_pass). Your counfiguration properties should look like this:

    --comp-name-1 = ext
    --comp-class-1 = tigase.server.ext.ComponentProtocol
    --external = muc.devel.tigase.org:muc-secret:listen:5270, \
        pubsub.devel.tigase.org:pubsub_pass, \
        msn.devel.tigase.org:msn_pass

Please note, the --external property with value should be written in a single line. Above example has split the line for readibility.

Prev | Up | Next
Chapter 60. Basic Configuration Options (External Component) | Home | More TCP/IP Ports