Chapter 15. --cm-ht-traffic-throttling
Prev |  | Next

# Chapter 15. --cm-ht-traffic-throttling

Artur Hefczyc <artur.hefczyc@tigase.net> v2.0, June 2014: Reformatted for AsciiDoc. :toc: :numbered: :website: http://tigase.net/ :Date: 2013-02-09 21:38

Default value: `xmpp:25k:0:disc,bin:200m:0:disc`

Example: `--cm-ht-traffic-throttling = xmpp:25k:0:disc,bin:200m:0:disc`

Possible values: comma separated list of traffic limits settings.

Description: The property is used to specify traffic limit of non-user connections, that is s2s, external components and other high traffic server connections. Meaning of the property and values encoded are in the same way as for the --cm-traffic-throttling property.

Available since: 5.1.3

Prev |  | Next
Chapter 14. --cluster-nodes | Home | Chapter 16. --cm-see-other-host