Configuration
Prev | Chapter 23. Tigase Push Component | Next

## Configuration

### Enabling component

Push notifications may be sent by Tigase XMPP Server with or without use of Push component. Push Component is only required if you have your own application for mobile devices for which you want to send push notifications.

This component is not loaded and enabled by default as it requires implementations of Push notifications providers and additional configuration (including credentials required to authorize to push services). Following entries will activate component:

    push () {
    }

### Note

You need to enable and configure push providers implementations before it will be possible to send push notifications. For more details about this process, please check documentations of push service provider projects.

Prev | Up | Next
Chapter 23. Tigase Push Component | Home | Usage