Chapter 15. --cm-ht-traffic-throttling
Prev |  | Next

# Chapter 15. --cm-ht-traffic-throttling

Default value: xmpp:25k:0:disc,bin:200m:0:disc

Example: --cm-ht-traffic-throttling = xmpp:25k:0:disc,bin:200m:0:disc

Possible values: 'comma separated list of traffic limits settings.'

Description: This property is used to specify traffic limit of non-user connections, that is s2s, external components and other high traffic server connections. The meaning of the property and values encoded are in the same way as for the --cm-traffic-throttling property.

Available since: 5.1.3

Prev |  | Next
Chapter 14. --cluster-nodes | Home | Chapter 16. --cm-see-other-host