Chapter 32. --monitoring
Prev |  | Next

# Chapter 32. --monitoring

Default value: 'none'

Example: --monitoring = jmx:9050,http:9080,snmp:9060

Possible values: 'list of monitoring protocols with port numbers.'

Description: This property activates monitoring interfaces through selected protocols on selected TCP/IP port numbers. For more details please refer to the monitoring guide in the user guide for details.

Available since: 4.0.0

Prev |  | Next
Chapter 31. --max-queue-size | Home | Chapter 33. --net-buff-high-throughput