Chapter 18. --cmpname-ports
Prev |  | Next

# Chapter 18. --cmpname-ports

Artur Hefczyc <artur.hefczyc@tigase.net> v2.0, June 2014: Reformatted for AsciiDoc. :toc: :numbered: :website: http://tigase.net/ :Date: 2013-02-09 21:42

Default value: depends on component.

Example: `--s2s-ports=5269,5270,5271`

Possible values: comma separate list of TCP/IP port numbers.

Description: The property is used to set ports list for a connection manager. cmpname is a component name of the connection manager you want to change ports numbers for. list of ports is a comma separated list of ports numbers. For example for the server to server connection manager named s2s the property would like like the example below:

    --s2s-ports=5269,5270,5271

Available since: 3.0.0

Prev |  | Next
Chapter 17. --cm-traffic-throttling | Home | Chapter 19. --comp-class