Chapter 15. HTTP File Upload component
Prev | Part I. Tigase Administration Guide | Next

## Chapter 15. HTTP File Upload component

Tigase’s HTTP File Upload component is an implementation of XEP-0363 HTTP File Upload specification. This allows file transfer between XMPP clients by uploading a file to HTTP server and sending only link to download file to recipient.

This implementation makes use of the HTTP server used by Tigase XMPP Server and Tigase HTTP API component to provide web server for file upload and download.

By default this component is disabled and needs to be enabled in configuration file before it can be used. Another requirement is that the proper database schema needs to be applied to database which will be used by component.

## Enabling HTTP File Upload Component

Configuration.

    upload() {}

Prev | Up | Next
Tigase Web Client | Home | Metadata repository